#
# $Header: /usr/local/monitoring/nagios/etc/services/RCS/netapp-services.cfg,v 1.6 2014/07/28 18:35:00 nagios Exp $
#
# NetApp services
#

define service {
	service_description		netapp_failed_fans
	use				generic-service-active
	hostgroup_name			NAS
	normal_check_interval		10
	retry_interval			5
	check_command			check_netapp_failed_fans
	contacts			NAS Admin
	contact_groups			null
}

define service {
	service_description		netapp_cf_settings
	use				generic-service-active
	hostgroup_name			NAS
	normal_check_interval		10
	retry_interval			5
	check_command			check_netapp_cf_settings
	contacts			NAS Admin
	contact_groups			null
}

define service {
	service_description		netapp_disk_space
	use				generic-service-active
	hostgroup_name			NAS
	normal_check_interval		10
	retry_interval			5
	check_command			check_netapp_disks
	contacts			NAS Admin
	contact_groups			null
}

define service {
	service_description		netapp_over_temp
	use				generic-service-active
	hostgroup_name			NAS
	normal_check_interval		10
	retry_interval			5
	check_command			check_netapp_over_temp
	contacts			NAS Admin
	contact_groups			null
}

define service {
	service_description		netapp_nvram
	use				generic-service-active
	hostgroup_name			NAS
	normal_check_interval		10
	retry_interval			5
	check_command			check_netapp_nvram
	contacts			NAS Admin
	contact_groups			null
}

define service {
	service_description		netapp_cf_partner_status
	use				generic-service-active
	hostgroup_name			NAS
	normal_check_interval		10
	retry_interval			5
	check_command			check_netapp_cf_partner_status
	contacts			NAS Admin
	contact_groups			null
}

define service {
	service_description		netapp_failed_disks
	use				generic-service-active
	hostgroup_name			NAS
	normal_check_interval		10
	retry_interval			5
	check_command			check_netapp_failed_disks
	contacts			NAS Admin
	contact_groups			null
}

define service {
	service_description		netapp_cpuload
	use				generic-service-active
	hostgroup_name			NAS
	normal_check_interval		10
	retry_interval			5
	max_check_attempts		4
	check_command			check_netapp_cpuload!90!95
	contacts			NAS Admin
	contact_groups			null
}

define service {
	service_description		netapp_cf_state
	use				generic-service-active
	hostgroup_name			NAS
	normal_check_interval		10
	retry_interval			5
	check_command			check_netapp_cf_state
	contacts			NAS Admin
	contact_groups			null
}

define service {
	service_description		netapp_global_status
	use				generic-service-active
	hostgroup_name			NAS
	normal_check_interval		10
	retry_interval			5
	check_command			check_netapp_miscGlobalStatus!3!3
	contacts			NAS Admin
	contact_groups			null
}

define service {
	service_description		netapp_cf_interconnect_status
	use				generic-service-active
	hostgroup_name			NAS
	normal_check_interval		10
	retry_interval			5
	check_command			check_netapp_cf_interconnect_status
	contacts			NAS Admin
	contact_groups			null
}

define service {
	service_description		netapp_failed_psu
	use				generic-service-active
	hostgroup_name			NAS
	normal_check_interval		10
	retry_interval			5
	check_command			check_netapp_failed_psu
	contacts			NAS Admin
	contact_groups			null
}

define service {
	service_description		netapp_disk_space_dba
	use				generic-service-active
	hostgroup_name			NAS
	normal_check_interval		10
	retry_interval			5
	check_command			check_netapp_disk_space!dba.cfg
	contacts			DBA Important
	contact_groups			null
}


